Connect the bme280

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **Function** | **Raspberry Pi** | **BME280** |
| 3.3 vdc power | Board pin 1 | VCC - Red |
| Ground | Board pin 6 | GND - Black |
| SCL | Board pin 5. BCM 3 | SCL - Yellow |
| SDA | Board pin 3. BCM 2 | SDA - Blue |
| 5 vdc | NOT from gpio. Use a separate battery |  |
| Servo vcc |  |  |
| Servo ground |  |  |
| Servo signal |  |  |

